# 5.1. Output settings

NOTE: before starting the configuration of the device it is necessary to press the button CONNECT or READ SETTINGS. If this is not done your parameters may be lost and it might be necessary to reset factory default settings. NOTE: to make your changes come into effect in the device you must press the button WRITE SETTINGS. NOTE: before starting configuration it is necessary to change the primary manufacturer password („0000“). Otherwise the device will ignore he commands sent from the computer.

| Output Number – the code number of specified output. Output Name – the code name/text of specified output. It is allowed to enter up to 16 simbols. In section Status indicate the specified outputs which will be activated.

| Using Module EPGM8 – Enable this function when module EPGM8 is used. The number of outputs will be increased to 12 units.

# 5.2. EPGM1 module

If module EPGM1 is attached to the system, use section EPGM1 Outputs for configurations. EPGM1 has 2 outputs which can be disabled/enabled at any time:
Remove Output - Disable a particular EPGM1 ouptute.
Remove All Outputs - Disable all EPGM1 outputs.
Restore - Enable a particular EPGM1 output selected from the Inactive Outputs in EPGM module drop-down list .