# 7. Scheduler Settings

NOTE: before starting the configuration of the device you must press the button CONNECT VIA USB or READ SETTINGS. If these actions are not completed your parameters can be lost and you might need to restore factory default settings. NOTE: to enable the changes in the device you must press the button WRITE SETTINGS.

Settings section Scheduler is intended for configuring automatic output control (see also 4. Control Parameters) and/or output control accessibility (see also 5. User Database) for the specified users accroding to time period and day (-s) of the week. You can set periods of time and frequency by weekdays for 8 different schedulers.
Scheduler No. – number of specified scheduler.
Start Hour / Start Min – time settings which represent starting time for specified automatic output control and/or output (-s) control by the specified user stored in the user database. The format – hour / minutes (first of all, set the date and time of the device – see chapter 3. Administration).
End Hour / End Min – time settings which represent ending time for specified automatic output control and/or output (-s) control by the specified user stored in the user database. The format – hour / minutes (device date and time must be set correctly – see chapter 3. Administration).
Mo/Tu/We/Th/Fr/Sa/Su – time settings which represents in which days speciffied automatic output control will be activated. Mo – monday, Tu– tuesday, We – wednesday, Th – thursday, Fr – friday, Sa – saturday, Su – sunday.
Always – function, activating automatic output control as soon as the specified event occurs.