# 3. Users

NOTE: before starting the configuration of the device it is necessary to press the button CONNECT or READ SETTINGS. If this is not done your parameters may be lost and it might be necessary to reset factory default settings. NOTE: to make your changes come into effect in the device you must press the button WRITE SETTINGS. NOTE: before saving the settings it is necessary to change the primary manufacturer password („0000“). Otherwise the device will ignore commands sent from the computer.

# 3.1. User data settings

Settings Users is used for putting authorized telephone numbers which will be used by the system EPIR for calling and/or delivering SMS messages in the case of alarm, the sequence starting with User1 and ending with User5, until the first successfully answered call or delivered message. Factory default value is none. The system EPIR allows entering 5 users (User1…User5) who will receive messages and will be able to change settings etc.

NOTE: the device will not call the other number on the list if the registered user picks up the phone or rejects the call. It is recommended for users to disable voice mail service on their telephones. If it is not disabled, in the case of alarm, when the system calls on user number voice mail can turn on in which case the call would not be diverted to another user number saved in the phone number list of the device.

It is necessary to enter only telephone number of the first user (User1), i. e. it is not necessarily to enter all 5 numbers (User1…User5) at once. User must type mobile number in the international format (it consist of only those digits that overseas callers must type: United Kingdom - 44[area code][local number]) without symbol '+'. E.g. the mobile number of user is +44 (0) 113 xxx xxxx, so the incorrectly and correctly entered numbers are:

## Incorrectly entered user number: 440113xxxxxxx or 0113xxxxxxx

## Correctly entered user number: 44113xxxxxxx

Additional settings are used: Arm/Disarm Event – When this function is enabled, the system sends SMS messages to the specified user informing about arm/disarm event after the user performs system arming/disarming. By default this feature is enabled for all users.
Alarm Event – When this function is enabled, the system sends SMS message to the specified user informing about system alarm event. By default this feature is enabled for all users.
Inform All about Arming/Disarming – When this function is enabled, the system sends information messages to all users about armed/disarmed security system. By default this function is disabled.
Keeper - Security Guard phone number. This user is able to receive SMS message informing about security system arming/disarming (Arm/Disarm Event chek-box must be enabled for this user) and/or in case of alarm (Alarm Event chek-box must be enabled for this user) only. System configuration or control from Keeper phone number is permanently disabled. SMS ALL – When this function is enabled, in the case of an alarm, the system simultaneously sends SMS messages to all entered users. By default this function is disabled. When this function is disabled, SMS messages are delivered in a sequence starting with the first user (User1). The message will be sent to the next user only in the case the device does not receive a confirmation about a successful SMS message delivery to the first recipient.
CALLS Enable - function enabling (check mark is selected) or disabling (check mark is not selected) calls to the specified users in the case of alarm. By default this function is enabled. SMS Enable - function enabling (check mark is selected) or disabling (check mark is not selected) SMS message delivery to the specified users in the case of alarm. By default this function is enabled.

# 3.2. Setting the main password

| When configuring or controlling the system by phone via SMS messages all sent commands start with a password, therefore you must memorize it. Manufacturer default password is 0000, which is necessary to change. In the environment of Configuration Tool you can do this in the section Users > Security, where you will have to enter your own password consisting of 4 digits. Having entered the desired password do not forget to save the settings (to press the button Write Settings). Allow Only preset Users - function, enabling (check mark is selected) the mode when the system reacts to the SMS messages - commands that are sent only from registered telephone numbers (User1...User5). If this function is disabled (check mark is not selected), the device can be controlled by all users who know the number of the SIM card inserted in the device, control commands and the password. By default this function is enabled.

NOTE: it is necessary to change default password (0000) because in the case the password is not changed the chosen parameters will not be stored in the device. NOTE: when entering the new password you cannot use full stops, colons and spaces. NOTE: even if you forgot the password using this software you will be able to easily check the password - all device settings, including the password, are displayed on the computer screen.

# 3.3. Selecting the language

Security system EPIR communicates with the user via SMS messages, which are used for sending various informational messages about system status. For the sake of comfort the user has an option to choose the language in which the SMS messages will be delivered. In Configuration Tool program environment you can quickly set the language in the section Users > Language choosing one of the possible variants:

| Lithuania - Lithuanian language; Russia - Russian language; English - English language; Eesti - Estonian language; Latviesu - Latvian language; Icelandic - Icelandic language; Greek - Greek language; Deutsch - Deutsch language; Finnish - Finnish language; French - French language; Spanish - Spanish language; Slovak - Slovak language; Czech - Czech language;

# 3.4. Periodical test settings

Security system EPIR can periodically send informational messages about device status, i. e., it informs the user about connection status, whether the security is armed/disarmed etc. every day at the preset time. This is the test how the system operates. The user can specify the frequency and time of these continuous messages:

| Period - specifies after how many days repetitive informational messages are delivered, e. g. if you enter "1" - the system sends messages every day, if you enter "2" - it sends messages every two days etc. Time - specifies the time at which informational message will be delivered, e.g.: if you specify "11" - the message will be delivered at 11:00 etc.

NOTE: the user can disable the function of delivering periodical informational messages if he/she fills the fields in sections Period and Time with zeros. NOTE: if you want system checks to be performed more often than once per day enter "0" in the section Period and "1...23" in the section Time. For instance, continuous check will be performed every two hours if you specify the following parameters: Period - "0", Time - "2".

# 3.5. Time and date settings

EPIR device has an integrated clock that must be set by the user when the device is started for the first time. The clock is intended for the system to send specific informational messages about system status at the specified time. You need to enter the following data:

| Date - date, the format: year-month-day; Time - time, the format: hours:minutes; In the environment of Configuration Tool the user can enter date and time data or automatically set this information according to computer clock (pressing the button Get PC Time). When all data is set you must press the button Set Clock - the time settings will be entered on the device.

NOTE: when device power supply gets cut off or the backup battery is depleted internal clock is restored to the previous factory default value. To have the system operate correctly you need to reset the internal clock of the device accordingly. NOTE: Configuration Tool program cannot read the internal clock of EPIR device, therefore when connecting the device to the software date and time fields will remain empty even though the time is set correctly in the device.