# 4. Valdymo parametrai

PASTABA: Prieš pradedant konfigūruoti įrenginį, būtina paspausti mygtuką CONNECT arba READ SETTINGS. Jei tai nebus padaryta - Jūsų parametrai gali būti sugadinti ir gali prireikti atstatyti gamyklinius parametrus. PASTABA: Norėdami, kad Jūsų pakeitimai įsigaliotų įrenginyje, būtina paspausti mygtuką WRITE SETTINGS. PASTABA: Būtina pakeisti gamintojo paliktą pradinį slaptažodį („0000“) prieš atliekant konfigūracijas. Kitu atveju, įrenginys ignoruos siunčiamas komandas iš kompiuterio.

# 4.1. Zonų identifikavimas

Naudojant daugiau nei vieną apsaugos sistemos EPIR įrenginį, kurie yra išdėstyti skirtingose teritorijose, vartotojui patogu juos pavadinti skirtingais kodiniais pavadinimais. Pavyzdžiui, įjungus vieną įrenginį namuose, o kitą įtaisius sandėliuke juos galima įvardinti atitinkamai „Kambarys“ ir „Sandėlys“. Tuomet apsaugos aliarmo atveju vartotojas tiksliai žinos kur yra įsilaužta ir galės atitinkamai veikti.

| Programos Configuration Tool aplinkoje nurodyti prijungto prie kompiuterio EPIR įrenginio pavadinimą galite Control > Zone Status skiltyje ties Zone1 eilute. Galite įvesti iki 25 simbolių.

Also security system EPIR zones can be configured to work in any of the following modes:

- Follow – this type of zone doesn't react and cause an alarm if activated during Delay mode (delay time to enter security code and disarm the system).
- Instant – this type of zone immediately cause an alarm if it is activated. Usually this type of zones is used for doors, windows and other detectors.
- Delay – this type of zone doesn't react to activation for 15 seconds and this time is set to disarm system via keypad. Also this type of zone are usually used to connect contacts of entry doors. When Delay zone isn't violated during arming process the system enters into Stay mode.
- 24H – this type of zone is used to connect sensors which must be monitored all the time, even when system is disarmed. Mostly these zones are used to connect tampers which detects when PIR or security panel box is opened.
- Fire – this type of zone is used to connect smoke detectors and monitors all the time even if the system is disarmed. Fire zone alarm is pulse (with pauses).
- Silent – this zone works as 24H zone and when it is violated, the system doesn't turn on the siren.

# 4.2. Virtual Zones

Virtual zones is used to virtually trigger system alarm and for test purposes. User can create virtual zone anytime if there is still empty spots for zones (system can handle up to 44 zones, which includes zones on board, wireless, virtual and EPGM zones).
Virtual zone is configurable in the same way as any other zone (zone on board, wireless and etc.) in the system. To create new virtual zone, press button Create New.... To remove virtual zone, select appropriate zone in virtual zones table and press button Remove Selected.
Zone Number – the code number of specified zone.
Zone Name – the code name/text of specified zone. If the specified zone is triggered, system sends to the user SMS message with the entered value. It is allowed to enter up to 24 symbols.
In the section Status it is indicated which zone will be activated (ON state) or deactivated (OFF state).
All security system ESIM264 zones can be configured to work in any of the following modes, which are represented in section Zone Type.
Entry Delay, s – This field is used to configure time which is dedicated to disarm the security system when users enters in the specified Delay zone. If system will not be disarmed in time, then it will cause an alarm. By default, this time is 15 seconds. This parameter can be adjusted only for Delay type zones.

# 4.3. Įrenginio valdymo parametrai

| Level – detektoriaus jautrumo lygio nustatymas. Galite įvesti reikšmes nuo 20 iki 99, kur atitinkamai mažesnis skaičius reiškia didesnį detektoriaus jautrumo lygį, t. y. įvedus 20 – nustatysite didžiausią jautrumo lygį, o įvedus 99 – nustatysite mažiausią galimą jautrumo lygį. Gamykloje nustatyta reikšmė yra 40. Alarm Time – Mažiausias laikas tarp pakartotinio aliarmo. Nurodo po kiek laiko vėl bus siunčiamos informacinės žinutės ir daromi skambučiai pakartotinio apsaugos aliarmo atveju. Naudojamas laiko vienetas yra minutės. Gamykloje nustatyta reikšmė yra 1 minutė. Exit Time – laikas, skirtas išeiti iš saugomos patalpos, po kurio įsijungia apsaugos sistema. Laiko vienetas yra sekundės. Gamykloje nustatyta reikšmė yra 15 sekundžių. Nurodžius reikšmę „0“, EPIR apsaugos sistema įsijungs iš karto be užlaikymo. Low Battery report Enable - function enabling (check mark is selected) or disabling (check mark is not selected) the mode when the system sends informational SMS messages about the status of external power supply (its cut-off or reoccurrence). By default this function is enabled. Battery Trouble Report Enable - when this function is enabled, system automatically informs user in case the battery is strongly needed to be changed. Bell Squawk Enable - by enabling this feature the siren provides short beeps while the system is counting down the exit delay time (arming the security system). By default this parameter is disabled. This feature applies to wired sirens only. LED Indication Enable - when this function is enabled, system LED lights up whenever a movement is detected while security system is armed. By default this feature is disabled. Advanced configuration - funkcija, skirta adaptuoti EPIR prie specifinių skirtingų mobilaus ryšio operatoriaus tinklų. Naudojama tik esant nekorektiškam įrenginio veikimui. Tačiau vartotojui nepatartina keisti šiuose laukeliuose pateiktų parametrų – būtina pasitarti su gamintoju!! SMS Delivery report Enable - SMS delivery report is necessary that the system could indicate which user have received SMS message about alarm or not. Otherwise, system will send alarm message to all provided users. By default, this function is enabled.

| Device OFF - Device will be instantly turned off. Boot Mode - system activates boot mode by opening a new window with existing firmware file (.bin file). In this case user will be able to upgrade existing firwmare version to a newest one (it is needed to delete the existing file and put in the new .bin file). Attention: Advanced use only!!! Use only in case You received new firmware file from distributors!!!

# 4.3. Additional options

| LED Indication Enable EPIR indicates detection with LED even when the system security is activated. By default, this function is disabled. SMS Delivery report Enable sms delivery report is necessary that the system could indicate which user have received sms message about alarm or not. Otherwise, system will send alarm message to all provided users. By default, this function is enabled.