# 2.1. Prisijungimas

PASTABA: Prieš pradedant konfigūruoti įrenginį, būtina paspausti mygtuką CONNECT arba READ SETTINGS. Jei tai nebus padaryta - Jūsų parametrai gali būti sugadinti ir gali prireikti atstatyti gamyklinius parametrus. PASTABA: Norėdami, kad Jūsų pakeitimai įsigaliotų įrenginyje, būtina paspausti mygtuką WRITE SETTINGS.

Apsaugos ir valdymo sistemos ESIM264 parametrų nustatymui naudokite kompiuterį, USB A- Mini / USB B kabelį ir konfigūravimo programą Configuration Tool. Jungiant pirmą kartą prie tam tikro kompiuterio, reikia palaukti, kad automatiškai įsidiegtų naudojami draiveriai (3 žingsnis). Detalesnė šių veiksmų seka pateikta toliau:

1. Prijunkite ESIM264 prie pagrindinio maitinimo šaltinio. 2. Sujunkite USB kabeliu sistemos ESIM264 mini USB jungtį su kompiuterio USB jungtimi. Jei jungiate NE pirmą kartą prie naudojamo kompiuterio, praleiskite 3 ir 4 žingsnį. 3. Draiverių instaliavimas (kompiuteris atliks automatiškai). 4. Pasibaigus draiverių instaliavimui, turite atjungti USB kabelį ir iš naujo jį prijungti. 5. Paleiskite programą Configuration Tool. 6. Paspauskite CONNECT mygtuką. 7. Pagrindiniame programos lange turi atsirasti sistemos versijos numeris (ties Status ir Version žymenimis – kaip parodyta pateiktame pavyzdyje). Jei versijos numeris neatsirado, patikrinkite prievado nustatymus, kabelio teisingą prijungimą bei sistemos maitinimo šaltinio prijungimą. Taip pat programa negali matyti prijungto įrenginio, jei bandoma jungtis iš administratoriaus teisių neturinčio vartotojo („Account'o“). Išsprendus problemą, vėl paspauskite CONNECT. |

# 2.2. Remote Configuration

NOTE: in order to start remote configuration via GPRS, it is necessary that GPRS settings (ESIM264 -> Connection -> Advanced Configuration -> System -> GPRS Settings) is provided.

NOTE: In order to activate GPRS connection between device and the server, You must send specified SMS command ("xxxx stconfig", here xxxx - Your 4 digit SMS password) to the device. NOTE: Possible temporary GPRS connection problems if system is calling to users (in case of alarm and etc.) at the same time when GPRS connection is activated.

Choose Remote Configuration option in Connection window if You want to connect to ESIM264 via GPRS. Additionally, You will be asked to choose the GPRS connection type and other specified parameters:

GPRS connection between device and software selection - choose option "Connect to Remote Server" to connect to device via remote server or choose "Run TCP/IP Server" in order to connect to device directly (it is necessary to configure Your router*). * - it is necessary to configure the router as incoming data to your public IP address (router, port: 5000) must be transmited to Your computer (by local IP address and indicated port). |

Providing additional information - You will be asked to provide device IMEI (it will be received with SMS message) if software is connecting to Remote Server or choose Computer TCP Port number if software is going to run TCP/IP Server. |

Connecting to device - after connection with Remote Server is established or TCP/IP Server is activated, it can take up to 2-3 minutes while device connects to software "Configuration Tool". When device is connected successfully, software will ask for admin password (the same as SMS password) or indicates that configuration read is proceeding. |

After configuration read is successfull, You can start configurations for ESIM264.