# 3. Administration

NOTE: before starting the configuration of the device it is necessary to press the button CONNECT VIA USB or READ SETTINGS. If this is not done your parameters may be lost and it might be necessary to reset factory default settings. NOTE: to make your changes come into effect in the device you must press the button WRITE SETTINGS. NOTE: before starting configuration it is necessary to change the default password (0000). Otherwise the device will ignore he commands sent from the computer.

# 3.1. Administrator control parameters

Settings section of the settings Users is used for putting authorized telephone numbers for which the system ESIM120 will allow performing configurations, i. e., changing relay operation duration, entering/deleting user numbers, receiving system SMS messages or calls. By default when one of the inputs Z1-Z3 is triggered, SMS messages are delivered in the sequence starting with User1 and ending with User5, until the first successful SMS message delivery. It is also possible to configure the system so that SMS messages are simultaneously received by all administrators. It is necessary to enter only telephone number of the first user (User1), i. e. it is not necessarily to enter all 5 numbers (User1...User5) at once. User must type mobile number in the international format (it consist of only those digits that overseas callers must type: 44[area code][local number]) without symbol '+'. E.g. the mobile number of user is +44 (0) 113 xxx xxxx, so the incorrectly and correctly entered numbers are:

## Incorrectly entered user number: 440113xxxxxxx or 0113xxxxxxx

## Correctly entered user number: 44113xxxxxxx

Additional settings are used: Output No. (1 / 2 / BOTH) - function allowing to assign the relay (relay 1, relay 2 or both) controlled by the specified administrator phone number. SMS All - function, enabling (check mark is selected) the mode when, in the case input Z1-Z3 is triggered, informational SMS messages are simultaneously sent to all the administrators on Users list. By default this function is disabled (check mark is not selected) – in this case informational SMS messages are delivered in a sequence starting with the first administrator (User1). The message is sent to the next administrator only in the case the device does not receive a confirmation about a successful SMS message delivery to the recipient. Call Back Enable - function enabling (check mark is selected) or disabling (check mark is not selected) the short call to the user from system ESIM120 informing about successfully enabled relay. Enable Control From Any Number - function enabling (check mark is selected) or disabling (check mark is not selected) the mode when the system reacts to any user who is making a call regardless of whether his/her telephone number is stored on user database. User Database Enable - function enabling (check mark is selected) or disabling (check mark is not selected) the relay control from phone numbers stored in the database.

# 3.2. Setting the main password

| When configuring or controlling the system by phone via SMS messages all sent commands start with a password, therefore you must memorize it. Manufacturer default password is 0000, which is necessary to change. In the environment of Configuration Tool you can do this in the section Users > Security, where you will have to enter your own password consisting of 4 digits. Having entered the desired password do not forget to save the settings (to press the button Write Settings).

NOTE: it is necessary to change factory default password (0000). If the password is not changed the chosen parameters will not be stored in the device. NOTE: when entering the new password you cannot use full stops, colons and spaces. NOTE: even if you forgot the password having connected to Configuration Tool using this software you will be able to easily check the password - all device settings, including the password, are displayed on the computer screen.

# 3.3. Selecting the language

The system ESIM120 communicates with the user via SMS messages, which are used for sending various informational messages about system status. For the sake of comfort the user has an option to choose the language in which the SMS messages will be delivered. In Configuration Tool program environment you can quickly set the language in the section Users > Language choosing one of the possible variants:

| Lithuania - Lithuanian language; Russia - Russian language; English - English language; Eesti - Estonian language;

# 3.4. Configuring periodical testing

The system ESIM120 can periodically send informational messages about device status, i. e, it informs the user about connection status, whether the security is armed/disarmed etc. every day at the preset time. This is the test how the system operates. The user can specify the frequency and time of these continuous messages:

| Period - specifies after how many days repetitive informational messages are delivered, e. g. if you enter "1" - the system sends messages every day, if you enter "2" - it sends messages every two days etc. Time - specifies the time at which informational message will be delivered, e.g.: if you specify "11" - the message will be delivered at 11:00 etc.

NOTE: the user can disable the function of delivering periodical informational messages if he/she fills the fields in sections Period and Time with zeros. NOTE: if you want system checks to be performed more often than once per day enter "0" in the section Period and "1...23" in the section Time. For instance, continuous check will be performed every two hours if you specify the following parameters: Period - "0", Time - "2".

# 3.5. Setting the time and date of the device

ESIM120 device has an integrated clock that must be set by the user when the device is started for the first time. The clock is intended for the system to send specific informational messages about system status etc. at the specified time. You need to enter the following data:

| Date - date, the format: year-month-day; Time - time, the format: hours:minutes;

In the environment of Configuration Tool the user can enter date and time data or automatically set this information according to computer clock (pressing the button Get PC Time). When all data is set you must press the button Set Clock - the time will be entered on the device.

NOTE: when device power supply gets cut off and the backup battery is depleted internal clock is restored to the previous factory default value; to have the system operate correctly you need to reset the internal clock of the device accordingly. NOTE: Configuration Tool program cannot read the internal clock of ESIM120 device, therefore when connecting the device to the software date and time fields will remain empty even though the time is set correctly in the device.